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E-Rate FY 2026 Category 2 Eligible Technology Needs
For Sumter County Library System

Form 470 # 
Needs List Summary (Rev01) – Wesmark

	Structured Cabling & Accessories
	
	
	

	5.0
	
	Cat.6a Cable Drops, Re-wire 1 location, Wesmark Branch (certify to standard). Include removal of existing cabling. 
See attached floor location plans for details.
**Note: see Structured Cabling Note below.
	200
drops

	[bookmark: _Hlk125381032]5.1
	
	[bookmark: _Hlk125381331]48-Port Leviton or Panduit Modular Patch Panel, include needed RJ45 Jack Modules. Use Red for Public PP Locations, Green for Staff PP Locations and Blue for wireless access point PP Locations.
	8

	5.3
	
	Dual Sided Vertical cable managers for existing 42U 2-Post Rack.
	2

	5.4
	
	Power Pole, Ivory
	2

	5.5
	NP2
	Neat-Patch Cable Management Unit
	2

	5.6
	UP1
	Middle Atlantic 1 Space Utility Panel – or equivalent
	12

	6.0
	
	CAT6a Patch Cable Snagless, RJ45, 1ft Green
	60

	6.1
	
	CAT6a Patch Cable Snagless, RJ45, 1ft Red
	36

	6.2
	
	CAT6a Patch Cable Snagless, RJ45, 1ft Blue (for APs)
	7

	6.3
	
	CAT6a Patch Cable Snagless, RJ45, 5ft Blue (for APs)
	7

	6.4
	
	CAT6a Patch Cable Snagless, RJ45, 10ft Green
	40

	6.5
	
	CAT6a Patch Cable Snagless, RJ45, 10ft Red
	24

	6.6
	
	CAT6a Patch Cable Snagless, RJ45, 25ft Red
	1

	6.7
	
	CAT6a Patch Cable Snagless, RJ45, 25ft Yellow
	1

	
	
	
	

	Power (UPS) 
	
	
	

	7.0
	9PX1500RTN-L
	Eaton 9PX Double-Conversion UPS, 1350W, 120V, Networked, 2U
	1

	7.1
	PDU121506
	Eaton Basic PDU - 13 NEMA 5-15R Outlets
	1

	7.2
	OL2200RTXL2U
	CyberPower Smart App Online 2200 UPS
	2

	7.3
	PDU20M2F8R
	CyberPower Metered PDU, 1U
	1




Additional Notes: 
Include setup and installation for all listed equipment above, unless otherwise noted. Configure Aruba Central to manage all Aruba switches.

**Structured Cabling Note: 
Vendor site walkthrough is required. All structured cabling must be certified to category standard. Test results and as-built diagram must be provided at completion of project. Vendor must submit Personnel qualifications (certifications, longevity within the sector, etc.) with their proposal.

Re-cable location. Replace Category 5e cable and replace with Category 6a. Category 5e cabling must be removed/uninstalled. Leave existing cabling in place that is currently used for Voice. All new cabling will be pulled to the MDF location identified on floor plan diagrams. There will be separate patch panels for the Public Network, the Staff Network and Wireless Access Points. This cable breakdown for this project is subject to change. See accompanying cabling project floor plan diagram for locations.

UNIVERSAL SERVICE PROGRAM for Schools and Libraries (E-RATE)
To warrant consideration for an award of contract resulting from this Request for Proposal, vendors must participate in the Universal Service Program for Schools and Libraries (commonly known as “E-rate”). Vendors must be in good standing with the FCC and must have a valid SPIN (Service Provider Identification Number). The SPIN and Form 470 number must be included on the proposal. 
There are two methods, or “modes” of invoicing under the E-Rate Program: The vendor must use the Service Provider Invoicing (SPI) method for this project.
https://www.usac.org/e-rate/two-methods-of-invoicing/

Branch Location(s)
	Wesmark Branch
180 W. Wesmark Blvd
Sumter, SC 29150
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