
	Run for OS2
	distance (ft)

	HS building to Gym
	370

	A-Vault to R-203
	387

	R-203 to E-200
	133

	R-203 to R-103
	150

	R-203 to R-105
	150

	A-Vault to C-201
	370

	C-201 to C-100
	50

	C-201 to D-200
	97

	A-Vault to S-200
	280

	HS building to A-Vault (buried)
	1000



Each run is inside a building except for the HS runs. The original fiber for the HS to Gym has a dedicated conduit but the HS to A-Vault might be a direct burial.

1. I have a set of Ubiquiti Building-to-building Bridge XG that needs to be installed to connect the HS to A-Vault prior to the fiber being run.
2. 2 connections per run for failover 
3. 4 connections from R-203 to E-200
4. Junction points at R-203 and C-201 go straight to A-Vault via junction box
5. Ubiquiti SFP modules are required


